Memory transfer

ORG 000H

MOVA,#25H

MOVR0,#10H

MOVR1,#08H

MOVDPTR,#100H

UP:

CLR A

MOVCA,@A+DPTR

MOV@R0,A

INC R0

DJNZ R1,UP

HERE:SJMP HERE

ORG 100H

DB 10H,20H,30H,40H,50H,60H,70H,80H

END

o/p

manually put 100H

